DC Bridge Tests

1. ON-OFF functionality

Test on off switch

1. Fuse test
2. DC level test
3. Diode bridge temperature test

Flyback Controller Test

1. Isolated feed-back test
2. Power on test with external DC bus PS and external controller PS
3. Output voltage level test with loading